# URC Rules Summary-Rover

## Size,Weight and Power -(Requirements for mechanical design)

* Rover cannot be connected to another platform.
* Dimensions : 1.2 m X 1.2 m , No restriction on height
* Foldable parts are allowed.
* Max mass at time of operation - 50 kg
* Max mass of rover and all attachments - 70kg
* No air ingesting propulsion systems allowed.
* Must have a readily visible kill switch on the exterior of the rover.